| 1 | 2 | 3
--- | --- | --- | ---
2 |  | Physical & Mechanical Properties |
4 | 1)\nTemperature Range |  | -40\nto 105°C
6 | 2) Bend Radius |  | 10X Cable Diameter
8 | 3) Pull\nTension |  | 3.5\nLbs, Maximum
9 |  | Electrical Properties\n(For\nEngineering purposes only) |
11 | 1) Voltage Rating |  | 300 VRMS
13 | 2)\nInductance |  | 0.07 μH/ft, Nominal
15 | 3) Conductor DCR |  | 25 Ω/1000ft @20°C, Nominal